- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_LcdcConfigLidd Struct Reference
LCDC Data Structures

Configuration parameters for LCDC in LIDD mode. More...

`#include <csl_lcdc.h>`

## Data Fields
Uint16 | clkDiv
CSL_LcdcFdoneCtl | fdoneIntEn
CSL_LcdcChipSelect | dmaCs0Cs1
CSL_LcdcDmaCtl | dmaEnable
CSL_BitMask16 | polControl
CSL_LcdcLiddMode | modeSel

## Detailed Description

Configuration parameters for LCDC in LIDD mode.

Used to configure LCDC for LIDD mode

## Field Documentation

Uint16 CSL_LcdcConfigLidd::clkDiv

Clock divisor (2-255)

CSL_LcdcChipSelect CSL_LcdcConfigLidd::dmaCs0Cs1

CS0/CS1 Select for LIDD DMA writes 0: DMA writes to LIDD CS0 1: DMA writes to LIDD CS1

CSL_LcdcDmaCtl CSL_LcdcConfigLidd::dmaEnable

LIDD DMA enable

CSL_LcdcFdoneCtl CSL_LcdcConfigLidd::fdoneIntEn

LIDD frame done interrupt

CSL_LcdcLiddMode CSL_LcdcConfigLidd::modeSel

LIDD Mode Select

CSL_BitMask16 CSL_LcdcConfigLidd::polControl

LIDD polarity control mask

The documentation for this struct was generated from the following file:

- csl_lcdc.h