- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
CSL_MMCCardIdObj Struct Reference
MMC/SD Data Structures

Card identification object. More...

`#include <csl_mmcsd.h>`

## Data Fields
Uint16 | mfgId
Uint16 | oemAppId
Uint8 | productName [6]
Uint16 | productRev
Uint32 | serialNumber
Uint16 | month
Uint16 | year
Uint16 | checksum

## Detailed Description

Card identification object.

## Field Documentation

Uint16 CSL_MMCCardIdObj::checksum

7 bit crc

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint16 CSL_MMCCardIdObj::mfgId

8 bit Manufacturer ID

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint16 CSL_MMCCardIdObj::month

4 bit Manufacturing Date (Month)

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint16 CSL_MMCCardIdObj::oemAppId

16 bit OEM and application ID

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint8 CSL_MMCCardIdObj::productName[6]

40 or 48 bit Product name

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint16 CSL_MMCCardIdObj::productRev

8 bit Product Revision Number

Uint32 CSL_MMCCardIdObj::serialNumber

32 bit Serial Number

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

Uint16 CSL_MMCCardIdObj::year

4 bit Manufacturing Date (Year) in case of MMC (Year 0 = 1997). SD has an 8 bit year field.(Year 0 = 2000)

Referenced by MMC_sendAllCID(), and SD_sendAllCID().

The documentation for this struct was generated from the following file:

- csl_mmcsd.h