
**** 05/30/23 12:09:26 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "SCHEMATIC1-bias"  [ C:\study\tps62933pspice-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\cds_spb_home\cdssetup\OrCAD_PSpiceTIPSpice_Install\17.4.0\PSpice.ini file:
.lib "nom_pspti.lib" 
.lib "nom.lib" 

*Analysis directives: 
.OPTIONS ADVCONV
.OPTIONS FILEMODELSEARCH
.PROBE64 V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source TPS62933PSPICE
X_U1         N15079 N14587 N16139 0 N14969 N14809 N15050 N14587 TPS62933_TRANS
+  PARAMS:  STEADY_STATE=0 EN_FSS=0
V_V1         N14587 0 24Vdc
C_C1         N15050 N15075  100n  TC=0,0 
C_C2         0 N14587  100n  TC=0,0 
C_C3         0 N14587  10u  TC=0,0 
C_C4         N14809 0  33n  TC=0,0 
C_C5         0 N15400  22u  TC=0,0 
C_C6         0 N15400  22u  TC=0,0 
C_C7         0 N15400  100n  TC=0,0 
C_C8         0 N14587  10u  TC=0,0 
R_R1         N14969 0  0 TC=0,0 
-----------------------$
ERROR(ORPSIM-16144): Value may not be 0
R_R2         N16135 N15400  49.9 TC=0,0 
R_R3         N16139 N16135  53.6k TC=0,0 
R_R4         0 N16139  10.2k TC=0,0 
R_RLOAD         0 N15400  5 TC=0,0 
R_R7         N15079 N15075  0 TC=0,0 
----------------------------$
ERROR(ORPSIM-16144): Value may not be 0
L_L1         N15050 N15400  6.8uH  

**** RESUMING bias.cir ****
.END
