U-Boot 2013.01 (Oct 02 2014 - 00:16:34)                                         
                                                                                
I2C:   ready                                                                    
Detected SO-DIMM [SQR-SD3T-2G1333SED]                                           
DRAM: 2 GiB                                                                     
                                                                                
Reseting entire DDR3 memory to 0 ...                                            
DRAM:  1 GiB                                                                    
NAND:  512 MiB                                                                  
Net:   K2HK_EMAC, K2HK_EMAC1, K2HK_EMAC2, K2HK_EMAC3                            
Hit any key to stop autoboot:  0                                                
K2HK EVM # env print                                                            
addr_fdt=0x87000000                                                             
addr_fs=0x82000000                                                              
addr_kern=0x88000000                                                            
addr_mon=0x0c5f0000                                                             
addr_secdb_key=0xc000000                                                        
addr_ubi=0x82000000                                                             
addr_uboot=0x87000000                                                           
addr_uinitrd=-                                                                  
args_all=setenv bootargs console=ttyS0,115200n8 rootwait=1                      
args_net=setenv bootargs ${bootargs} rootfstype=nfs root=/dev/nfs rw nfsroot=${p
args_ramfs=setenv bootargs ${bootargs} rdinit=/sbin/init rw root=/dev/ram0 initM
args_ubi=setenv bootargs ${bootargs} rootfstype=ubifs root=ubi0:rootfs rootflag8
args_uinitrd=setenv bootargs ${bootargs} rdinit=/sbin/init rw root=/dev/ram0    
baudrate=115200                                                                 
boot=ubi                                                                        
bootargs=console=ttyS0,115200n8 rootwait=1 rootfstype=ubifs root=ubi0:rootfs ro8
bootcmd=run init_${boot} get_fdt_${boot} get_mon_${boot} get_kern_${boot} run_mn
bootdelay=3                                                                     
bootfile=/K2/k2hk-evm-ubifs.ubi                                                 
burn_ubi=nand erase.part ubifs; nand write ${addr_ubi} ubifs ${filesize}        
burn_uboot=sf probe; sf erase 0 0x100000; sf write ${addr_uboot} 0 ${filesize}  
dnsip=192.0.2.2                                                                 
dnsip2=192.0.2.3                                                                
erase_nand_ubi=nand erase.part ubifs                                            
ethact=K2HK_EMAC                                                                
ethaddr=00:17:ea:f7:10:0e                                                       
fdt_high=0xffffffff                                                             
fileaddr=82000000                                                               
filesize=FC00000                                                                
get_fdt_net=dhcp ${addr_fdt} ${tftp_root}/${name_fdt}                           
get_fdt_ramfs=dhcp ${addr_fdt} ${tftp_root}/${name_fdt}                         
get_fdt_ubi=ubifsload ${addr_fdt} ${name_fdt}                                   
get_fdt_uinitrd=dhcp ${addr_fdt} ${tftp_root}/${name_fdt}                       
get_fs_ramfs=dhcp ${addr_fs} ${tftp_root}/${name_fs}                            
get_fs_uinitrd=dhcp ${addr_fs} ${tftp_root}/${name_uinitrd}                     
get_kern_net=dhcp ${addr_kern} ${tftp_root}/${name_kern}                        
get_kern_ramfs=dhcp ${addr_kern} ${tftp_root}/${name_kern}                      
get_kern_ubi=ubifsload ${addr_kern} ${name_kern}                                
get_kern_uinitrd=dhcp ${addr_kern} ${tftp_root}/${name_kern}                    
get_mon_net=dhcp ${addr_mon} ${tftp_root}/${name_mon}                           
get_mon_ramfs=dhcp ${addr_mon} ${tftp_root}/${name_mon}                         
get_mon_ubi=ubifsload ${addr_mon} ${name_mon}                                   
get_mon_uinitrd=dhcp ${addr_mon} ${tftp_root}/${name_mon}                       
get_ubi_net=dhcp ${addr_ubi} ${tftp_root}/${name_ubi}                           
get_uboot_net=dhcp ${addr_uboot} ${tftp_root}/${name_uboot}                     
has_mdio=0                                                                      
init_net=run set_fs_none args_all args_net                                      
init_ramfs=run set_fs_none args_all args_ramfs get_fs_ramfs                     
init_ubi=run set_fs_none args_all args_ubi; ubi part ubifs; ubifsmount boot;ubi;
init_uinitrd=run set_fs_uinitrd args_all args_uinitrd get_fs_uinitrd            
initrd_high=0xffffffff                                                          
ipaddr=157.87.43.158                                                            
mem_lpae=1                                                                      
mem_reserve=512M                                                                
mtddevname=bootloader                                                           
mtddevnum=0                                                                     
mtdids=nand0=davinci_nand.0                                                     
mtdparts=mtdparts=davinci_nand.0:1024k(bootloader),512k(params)ro,522752k(ubifs)
name_fdt=uImage-k2hk-evm.dtb                                                    
name_fs=arago-console-image-k2hk-evm.cpio.gz                                    
name_kern=uImage-keystone-evm.bin                                               
name_mon=skern-k2hk-evm.bin                                                     
name_ubi=k2hk-evm-ubifs.ubi                                                     
name_uboot=u-boot-spi-k2hk-evm.gph                                              
name_uinitrd=uinitrd.bin                                                        
nand_erasesize=20000                                                            
nand_oobsize=40                                                                 
nand_writesize=800                                                              
netmask=255.255.254.0                                                           
nfs_options=v3,tcp,rsize=4096,wsize=4096                                        
nfs_root=/export                                                                
no_post=1                                                                       
partition=nand0,0                                                               
run_kern=bootm ${addr_kern} ${addr_uinitrd} ${addr_fdt}                         
run_mon=mon_install ${addr_mon}                                                 
serverenv=print serverip                                                        
serverip=157.87.43.50                                                           
set_fs_none=setenv addr_uinitrd -                                               
set_fs_uinitrd=setenv addr_uinitrd ${addr_fs}                                   
size_ubi=0xfc00000                                                              
stderr=serial                                                                   
stdin=serial                                                                    
stdout=serial                                                                   
tftp_root=/K2                                                                   
ver=U-Boot 2013.01 (Oct 02 2014 - 00:16:34)                                     
write_nand_ubi=nand write ${addr_ubi} ubifs ${size_ubi}                         
                                                                                
Environment size: 3564/262140 bytes                
