MSP Gas Metering Library

- Main Page
- Introduction
- Usage
- Modules
- Data Structures
- Disclaimer

- Data Structures
- Data Structure Index
- Data Fields

Data Structures
Here are the data structures with brief descriptions:

GASMETERING_Algorithms_Configuration | This structure allows to configure the Time of Flight Algorithm
GASMETERING_Algorithms_Results | This structure is used by GASMETERING_runAlgorithms to return the results for Abs ToF, Delta ToD and Volume Flow Rate calculations
GASMETERING_configuration | This is the Gas Metering configuration structure. All expect a a pointer to this configuration structure. The Application will define this structure via the configuration files of the library
GASMETERING_HAL_functions | This structure is use to provide the pointer to Gas Metering HAL functions
GASMETERING_handle | This hanlde is initialized when calling GASMETERING_configureUltrasonicMeasurement and GASMETERING_intializeAlgorithm
GASMETERING_Measurement_Configuration | This structure allows the user to configure firing and capture setting
GASMETERING_Meter_Configuration | This structure allows user to provide Gas Meter configuration parameters
GASMETERING_Status_Flags | The following structure contains all status flags used by the library
GASMETERING_System_Configuration | This structure allows user to provide System Configuration parameters